From 688a01284ba4dd2f97c581f019f0cdedd0329525 Mon Sep 17 00:00:00 2001
From: Refik Hadzialic
Date: Wed, 23 May 2012 15:23:53 +0200
Subject: Config

---
 vorlagen/thesis/src/kapitel_A.tex | 22 ++++++++++++++++++----
 1 file changed, 18 insertions(+), 4 deletions(-)

(limited to 'vorlagen/thesis/src/kapitel_A.tex')

diff --git a/vorlagen/thesis/src/kapitel_A.tex b/vorlagen/thesis/src/kapitel_A.tex
index e169494..e526daa 100644
--- a/vorlagen/thesis/src/kapitel_A.tex
+++ b/vorlagen/thesis/src/kapitel_A.tex
@@ -63,6 +63,7 @@ autoreconf -fi
 make
 sudo make install
 sudo ldconfig
+cd ..
 \end{lstlisting}
 
 After the previous steps have finished successfully, the author will
@@ -76,12 +77,25 @@ sudo export PKG_CONFIG_PATH=/usr/local/lib/pkgconfig
 make
 \end{lstlisting}
 
-At this point, OpenBSC should be successfully installed. 
+At this point, OpenBSC should be successfully compiled. 
 \newpage
-\subsection{Configuring OpenBSC for nanoBTS}
-To enable the nanoBTS and OpenBSC to be fully operational the last configuration
+\subsection{Configuring nanoBTS for OpenBSC}
+To enable the nanoBTS and OpenBSC to be fully operational, the last configuration
 steps have to be made. We need to find and select a free channel in the GSM
-frequency band where our system is supposed to work. 
+frequency band where our system is expected to work. It is necessary to set
+the IP address of the server running OpenBSC on the nanoBTS as well. 
+
+We need to create the directory where the configuration file
+will be located and to modify the configuration file.
+\begin{lstlisting}[backgroundcolor=\color{light-gray}][numbers = none]
+sudo mkdir /usr/local/lcr
+cd ~/gsm_localization/openbsc/openbsc/doc/
+cd examples/osmo-nitb/nanobts 
+sudo cp openbsc.cfg /usr/local/lcr
+\end{lstlisting}
+
+
+
 \newpage
 \subsection{Installing RRLP software}
 \newpage
-- 
cgit v1.2.3-55-g7522

