From c7eb5bfddce3f50de7c72ad1d98c2fc7d3a7a14d Mon Sep 17 00:00:00 2001
From: Refik Hadzialic
Date: Mon, 9 Apr 2012 18:52:07 +0200
Subject: das

---
 vorlagen/thesis/src/kapitel_x.tex | 19 ++++++++++++++++---
 1 file changed, 16 insertions(+), 3 deletions(-)

(limited to 'vorlagen/thesis/src/kapitel_x.tex')

diff --git a/vorlagen/thesis/src/kapitel_x.tex b/vorlagen/thesis/src/kapitel_x.tex
index 1727864..3d05e00 100644
--- a/vorlagen/thesis/src/kapitel_x.tex
+++ b/vorlagen/thesis/src/kapitel_x.tex
@@ -176,9 +176,22 @@ which are serial communication interfaces.
 
 \section{Cable configuration}
 \label{sec:hardwareConfig}
-In the next section, the author will focus on connecting the hardware properly. 
-At least 4 network ethernet cables were required and one switch or hub connected
-to the internet. 
+In the next section, the author will focus on properly connecting the hardware. 
+At least 4 ethernet cables with RJ45 connectors, on both sides, were required
+and one switch or hub connected to the internet. One should
+take notice of the cabling between the nanoBTS and the ethernet switch or hub,
+since wrong cabling with the power supply unit (PSU) could damage one of
+the devices. In Figure \ref{img:connectionDiagram}, the junction points are
+label according to the used configuration setting. The ethernet cables
+between the switch/hub, PSU and nanoBTS should not be longer
+than 100 m \citep{installnanoBTS}.
+
+\begin{figure}[ht!]
+  \centering
+  \includegraphics[scale=0.5]{img/hardwareConnection}
+  \caption[]{Cable connections, showing interconnection diagram}
+\label{img:connectionDiagram}
+\end{figure}
 
 \chapter{Implementation}
 
-- 
cgit v1.2.3-55-g7522

